{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Przedmiar-obmiar robót"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Przedmiar-obmiar robót","index":0,"n_rows":24,"n_cols":5,"rows_kept":24,"cut":false,"hidden":false,"merged":[[3,2,3,3],[4,1,4,3],[5,1,5,3],[6,0,7,0],[6,1,7,1],[6,2,6,3],[8,0,9,0],[8,1,9,1],[8,2,8,3],[10,0,11,0],[10,1,11,1],[10,2,10,3],[12,0,13,0],[12,1,13,1],[12,2,12,3],[14,0,15,0],[14,1,15,1],[14,2,14,3],[16,0,17,0],[16,1,17,1],[16,2,16,3],[18,0,19,0],[18,1,19,1],[18,2,18,3],[20,0,21,0],[20,1,21,1],[20,2,20,3],[22,0,23,0],[22,1,23,1],[22,2,22,3]],"flags":["formulas_cached_only"]}
[]
[]
[]
["Lp","Normatyw","Opis",null,"Suma"]
[1,"Obiekt: Przedszkole Publiczne w Połańcu - Filia Nr 1 ul. Żapniowska 1"]
[" 1. 1.","   Element: Sale dydaktyczne:  - dwie sale"]
[" 1. 1. 1.","KNR\n04-01-0816-0600","Rozebranie posadzek z deszczułek z oderwaniem listew lub cokołów\n(5,90 x 11,75) x 2sale x 5%\n[ 6.9000 ]\n",null,6.9]
[null,null,"Jm. m2","Razem:",6.9]
[" 1. 1. 2.","KNR\n02-02-1111-0100","Posadzki z deszczułek na lepiku\n(5,90 x 11,75)m x 2sale x 5%\n[ 6.9000 ]\n",null,6.9]
[null,null,"Jm. m2","Razem:",6.9]
[" 1. 1. 3.","KNNR-W\n00-03-0807-0400","Mechaniczne cyklinowanie posadzek z deszczułek w pomieszczeniach ponad 8 m2\n(5,90 x 11,75))m x 2sale\n[ 138.7000 ]\n",null,138.7]
[null,null,"Jm. m2","Razem:",138.7]
[" 1. 1. 4.","KNR\n02-02-1111-0800","Lakierowanie posadzek i parkietów\n(5,90 x 11,75)m x 2sale\n[ 138.7000 ]\n",null,138.7]
[null,null,"Jm. m2","Razem:",138.7]
[" 1. 1. 5.","KSNR\n00-03-0605-0400","Dwukrotne malowanie tynków wewnętrznych ścian i sufitów farbą emulsyjną z przygotowaniem powierzchni - dwie sale\nsufity - 138.70m2\nściany - 95.90m2\n[ 234.6000 ]\n",null,234.6]
[null,null,"Jm. m2","Razem:",234.6]
[" 1. 1. 6.","KSNR\n00-03-0605-0600","Dwukrotne malowanie tynków wewnętrznych farbą olejną z jednokrotnym szpachlowaniem - dwie sale\n38.97m2 x 2\n[ 77.9000 ]\n",null,77.9]
[null,null,"Jm. m2","Razem:",77.9]
[" 1. 1. 7.","KNR-W\n04-01-1209-0800","Dwukrotne malowanie farbą olejną uprzednio malowanej stolarki drzwiowej, ścianek i szafek o pow. ponad 1.0 m2 \nstolarka drzwiowa - 7.20m2 x 2sale\n[ 14.4000 ]\n",null,14.4]
[null,null,"Jm. m2","Razem:",14.4]
[" 1. 1. 8.","KNNR-W\n00-03-1011-0300","Lakierowanie powierzchni drewnianych i metalowych gładkich -  zabudowa grzejników\n(0.90 x 2.40 x 6) x 2sale\n[ 25.9000 ]\n",null,25.9]
[null,null,"Jm. m2","Razem:",25.9]
[" 1. 1. 9.","KNR-W\n04-01-1212-2800","Dwukrotne malowanie farbą olejną rur wodociągowych i gazowych o śr.do 50 mm - 2 sale\n(12,60 + 6,00mb) x 2\n[ 37.2000 ]\n",null,37.2]
[null,null,"Jm. m","Razem:",37.2]